MAX9778 pin settings

Gain for amps: set to 2 for gain a and then 2.5 for gain b

Aux jack should be 2.2 volts peak to peak max so gain of 1->2 should keep us within 5v range

Gain is Rf/Rin

Follow typical application 2 for bast boosting and cap values 🡨 keep this

Gain for typical application is 1 for a and over 2 for b 🡨 keep this

Follow typical applications for most

Set INL2 and INR2 to be grounded through 15k resistor and cap